n Thermal head is worn out for printer 1 (715-0001, 815-0001, 1015-0001)

Error content | Thermal head is worn out for printer 1.
Detail | Affected content is separated by sub-error number. 0001: The portion that as run-out has no effect on printing.
Solution | Press [EXEC] or [STOP] button. [EXEC]: Head check is performed to the next product. [STOP]: Head check is not performed to the next product.
Action by user |
Action by service representative |
Related part |
Remarks | Printer number is changed depending on error number. Illustration of indicator is displayed by type of models.