- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Go back to original position (0322)

Error content | Displayed the condition of the under labeller printer.
Detail | Under labeller roller is getting out when indicated upper side of the under labeller printer. Under labeller unit is putting out when indicated middle of the under labeller printer. Label is not peeling off when indicated lower side of the under labeller printer.
Solution | Press [RETURN] button.
Action by user | Press [RETURN] button.
Action by service representative | Press [RETURN] button.
Related part |
Remarks |