- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Label is remaining (0312)

Error content | Label is remaining
Detail | Separated by sub-error number. 0000: Printer
Solution | Remove label and press [OK] button.
Action by user | Remove the label of the printer.
Action by service representative | Confirm the peel sensor operation of the printer on which an error occurred.
Related part | Main board, printer board
Remarks | Printer No.1, 2

Error content | Label is remaining on applicator
Detail | Separated by sub-error number. 0000: Applicator
Solution | Remove the label on applicator, Press [OK] button.
Action by user | Remove the label of the printer.
Action by service representative | Confirm the operation of the printer sensor.
Related part | Printer board
Remarks | Only for POP printer