- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Go back to original position (0322)

Error content | Displayed the condition of POP printer.
Detail | Label is remaining on POP applicator when indicated upper side of POP printer. Label is not peeling off when indicated lower side of POP printer.
Solution | Press [RETURN] button.
Action by user | Press [RETURN] button.
Action by service representative | Press [RETURN] button.
Related part |
Remarks |