- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No response from wrapper (402)

Error content | There was no response with respect to the inquiry conducted by the main board to the wrapper board P-1105 [A200] about the state.
Detail | This is a communication error that has occurred after performing power-on processing. The sub-error includes the communication phase number.
Solution | Press [STOP] to release the error. Press [REEXEC] to check the connection with the wrapper again.
User’s action | Turn off the power supply and then turn on the power supply again.
Service person’s action |
Related part | ① P-1105 [A200] XJ26 ② DC 24V supply to the power supply (XJ12) of P-1105 [A200] (DC 24V is normally supplied when the LED of P-1105 [A200] is lit.) ③ RS485 communication cable between the main board (P-1100, P-1163, P-1000) [A10] and P-1105 [A100, A200, A300] The following RS485 communication has not been established: Between P-1163 [A10] (XJ4) and P-1105 [A100] (XJ26) Between P-1105 [A100] (XJ27) and P-1105 [A300] (XJ26) Between P-1105 [A300] (XJ27) and P-1105 [A200] (XJ27)
Remarks | Pricing is only possible after the [STOP] button is pressed.