- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Control board for printer 1 is failed (717-0000, 817-0000)

Error content | Control board for printer 1 is failed (No.1: P-1163, No.2: P-1001).
Detail | Unable to detect an interrupt signal from the printer control board (P-1163, P-1001).
Solution | Restore power
Action by user |
Action by service representative |
Related part |
Remarks | “Printer No.1” changes depending on error No.