- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Wrong tray against programmed tray (476)

Error content | Tray settings and feed tray are different.
Detail | The wrapper detected the narrow-side dimensions of the feed tray are more than 50 mm larger than the selected tray. The narrow-side dimensions detected by the wrapper are shown in the sub-error.
Solution | [RETURN] button
Action by user | Clean up the sensor that detects products on the lift.
Action by service representative | Adjust the sensitivity of the sensor that detects products on the lift.
Related part | ① P-1105 [A200] ② Detection of products on the lift [B206]. ③ Feeder motor
Remarks |