- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Products are stuck on the stock conveyor (0315)

Error content | Products are stuck on the stock conveyor.
Detail | Occurs while the product blocks the full sensor from light when products remain on the discharge conveyer.
Solution | [OK] button, remove products on stock conveyor.
Action by user | Remove the product on the stock conveyor. * The error is cleared when the product is removed.
Action by service representative | Confirm the operation of the full sensor.
Related part | Main board, wrapping machine board
Remarks |