- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

Errror Number | Error Conternt
Normal | P Type | JW Type | BR Type
301 |  |  |  | Emergency switch has been pushed
303 |  |  |  | Front cover is open
305 |  |  |  | Infeed is slided
306 |  |  |  | Right film remove cover is open
307 |  |  |  | Left film remove cover is open
309 |  |  |  | Left film exchange cover is open
310 |  |  |  | Bracket for camera is up
312 | 312 |  |  | Label is remaining (0000)
312 | 312 |  |  | Label is remaining on applicator (0001)
| 312 |  |  | POP label is remaining (0002)
|  | 312 |  | Label is remaining (0004)
313 | 313 |  |  | Printer thermal head is up
315 |  |  |  | Products are stuck on the stock conveyor
316 |  |  |  | Mark down price is more than original price
318 |  |  |  | Mark down unit price is more than original price
319 |  |  |  | Production for target is completed
321 |  |  |  | Price is not programmed
322 | 322 | 322 |  | Go back to original position
325 |  |  |  | Weight is out of range (0000)
325 |  |  |  | Weight is out of range (0001)
326 |  |  |  | It cannot detect tray
327 |  |  |  | It cannot detect tray
328 |  |  |  | It cannot differentiate tray
333 |  |  |  | It cannot differentiate tray
334 |  |  |  | Tray is not programmed
335 |  |  |  | Close tray is programmed
336 |  |  |  | Completed production for order count
337 |  |  |  | Order is deleted
339 |  |  |  | Lower value is less than fixed weight
341 |  |  |  | Product is remaining on the lift
342 |  |  |  | POS code is not programmed
350 |  |  |  | Tray no. is not programmed
351 |  |  |  | Label is remaining
355 |  |  |  | Tray no. is not programmed
360 |  | 360 |  | Open the front cover
363 |  |  |  | It could not detect the tray
368 |  |  |  | Product is remaining
|  | 371 |  | Roller for under labeler is out
|  | 372 |  | Select DP mode
|  | 373 |  | Stock part is not set
|  | 374 |  | Use DP mode
|  | 375 |  | Use DP mode
|  |  | 395 | Auto feeder is not connected
396 |  |  |  | No USB memory
|  |  | 3017 | It cannot differenciate tray
|  |  | 3018 | Tray is placed in front