< Sum value for receiving is abnormal (1530)

Error content | Data sum value error when downloading the program
Detail | Occurs if error exists of program data received from detector board when downloading the detection application program. Communication was not achieved between the main board and detector board due to noise when downloading.
Solution | [OK] button
Action by user |
Action by service representative | Perform re-download of the detector application.
Related part | Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |