n Abnormal for sensor (POP label) (616-2040)

Error content | Abnormal for applicator sensor.
Detail | A sensor that does not have light blocked is blocked from light. Sub-error meaning is as follows: 2040: X axis
Solution | Press [RETURN] button.
Action by user |
Action by service representative |
Related part | (1) X-axis origin point of POP printer [B407] (2) Suction position of POP printer [B406]
Remarks |

###