- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Lower value is less than fixed weight (0339)

Error content | Lower value is less than fixed weight.
Detail | Attempted to enter a minimum value lighter than the fixed weight in fixed weight mode.
Solution | [EXEC] button => Set fixed weight to the minimum value. [STOP] button => Release error.
Action by user | Confirm [Fixed weight] and [Lower limit weight] of the product master.
Action by service representative | Confirm the product master. Confirm the host product master when linked with the host system.
Related part | Main board
Remarks | The minimum value will remain the same if the error is released.