< Cutter is not back to original position (481)

Error content | Cutter is not back to original position.
Detail | Cutter is not back to original position when starting cutter operation.
Solution | Press the [RETURN] button after checking for objects.
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 Origin point of cutter [B300]. 嘊 Cutter solenoid front [L300]. 嘋 Cutter solenoid rear [L301].
Remarks |