- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■ Automatic adjustment (1534)

Error content | Automatic adjustment for the detector.
Detail | A screen that indicates the detector is performing the automatic adjustment (brightness, distortion, volume). After the automatic adjustment, the screen changes to error screen for No.1535 or No.1537.
Solution |
Action by user |
Action by service representative |
Related part |
Remarks |