- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Product is remaining on the lift (0341)

Error content | Product is remaining on the lift.
Detail |
Solution | [OK] button
Action by user | Press the [OK] button to release the error screen, press the [PLU] key to discharge the product on the lift.
Action by service representative | Press the [OK] button to release the error screen, press the [PLU] key to discharge the product on the lift.
Related part | Main board, wrapping machine board
Remarks | Press the [PLU] button and remove the product after releasing the error.