< Blackout for the power (1504)

Error content | Tray detector detected power OFF in the console.
Detail | Power ON command received twice from the console.
Solution | Restore power
Action by user |
Action by service representative | Confirm the power supply 24 V DC of the main board (P-1100, P-1163, P-1000). RS485 communication line of the main board [A221 XJ-11].
Related part | Switching power supply [U10] Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |