< Centering motor is abnormal (422)

Error content | Centering motor error.
Detail | Centering motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 P-1006 board for tray press/centering [A202] 嘊 Centering motor [M205] 嘋 Centering origin [B205]
Remarks |