< Do not put your hands into the machine (448)

Error content | A hand was put into the wrapper during operation.
Detail | Occurs when a hand or object is detected entering the infeed conveyor while the wrapper is operating. 0000: A hand is detected entering the infeed conveyor in forward side. 0001: A hand is detected entering the infeed conveyor in backward side
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Hand insertion in the infeed conveyor <forward side> (light receiving/emitting) [B216]. 嘊 Hand insertion in the infeed conveyor <backward side> (light receiving/emitting) [B215].
Remarks |