< Wrong selection for big/small lift (475)

Error content | Wrong selection for big/small lift.
Detail | The rear feeder is in a position where it may come in contact with the lift when it is pushed up. Sub-error meanings are as follows: 0000 or 001*: Error occurs when small lift is selected (Not enough stretch). 0001 or 002*: Error occurs when large lift is selected (Lift selection is unsuitable or not enough stretch). * either 0,1, or 2
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part |
Remarks | Set the appropriate values for the lift selection and the stretch (fine adjustment) after cancelling the error.