- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Emergency switch has been pushed (0301)

Error content | Emergency switch has been pushed.
Detail | The emergency stop switch is pushed before operation. The emergency stop switch is blinking red on the wrapping unit display.
Solution | Release emergency stop switch, [OK] button.
Action by user | Release the emergency stop button.
Action by service representative | Release the emergency stop button.
Related part | Main board, wrapping machine board
Remarks |