< Product is on the lift (486)

Error content | Product is on the lift
Detail | There was a product on the lift when each of the following operations was started (completed). Sub-error meanings are as follows: 0000: After completion of returning operation. 0004: Wrapping the first product is attempted. 0007: Shifting to sleep mode. Others: Sending film or film loading is attempted.
Solution | Press the [RETURN] button after removing the product.
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Detection of products on the lift [B206].
Remarks |