- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No label for printer1 (710-0002, 810-0002)

Error content | Printer label finished.
Detail | Message indicates that labeling issue is completed in DP mode, and closing the front cover.
Solution | Replace the label by performing unloaded feed, close the front cover, then press the [RETURN] button or the [PLU] button.
Action by user |
Action by service representative |
Related part |
Remarks | “Printer No.1” changes depending on error No.