< Do not put your hands into the machine (449)

Error content | A hand was put into the wrapper during operation.
Detail | Occurs when a hand or object is detected entering the infeed conveyor while the wrapper is operating. Sub-error meanings are as follows: 0000: Detected by a sensor located over the outfeed heater. 0001: Detected by a sensor located under the cover.
Solution | Press the [RETURN] button after making sure a hand or object is not placed.
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100] 嘇 Hand insertion in the outfeeder (light receiving/emitting) [B106]: Sub-error is 0000. 嘊 Hand insertion in the front cover (light receiving/emitting) [B107]: Sub-error is 0001.
Remarks |