- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< It could not detect the tray (0363)

Error content | It could not detect the tray.
Detail | Occurs when a centered tray can't be detected normally. Occurs when a transparent tray is set to the above conditions.
Solution | Unstable, [EXEC] button.
Action by user | Place the tray again. Confirm the tray master. Press the [EXEC] button. Change the setting to [Centering: No].
Action by service representative | Confirm the tray master. Change the setting to [Centering: No].
Related part | Main board, detection board
Remarks |