- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Cover for the infeed is open (516)

Error content | The cover of the automatic infeeder has been opened.
Detail | The cover of the PS-AI was opened while the PS-AI was in operation (including the transfer standby state), or the user attempted to operate the PS-AI while the cover was open.
Release method | Open the cover, remove the product, and press the [RETURN] button.
User’s action | Open the cover, remove the product, and press the [RETURN] button.
Service action |
Relevant locations | P-1105[A600]
Remarks |