- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Tray is placed in front (521)

Error content | The tray is placed in front.
Detail | Before the wrapping operation, the product has shielded light at the tray front detection sensor.
Release method | Follow the on-screen instructions and press the [OK] button.
User’s action | When using PS-AI: Remove the product from the weighing platter and press the [START] button. When manually feeding products: Reposition the product.
Service action |
Relevant locations | 1) P-1105[A600] 2) Tray front detection sensor [B103]
Remarks |