- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< There is problem on wrapping controller (471)

Error content | Wrapper control board is abnormal.
Detail | An error occurred in the wrapper control board. Sub-error meanings are as follows: 0003: E2ROM writing error. 0088: IC for general-purpose communication error. 0999: High speed, external CPU reset interrupt.
Solution |
Action by user |
Action by service representative |
Related part | P-1105 [A100, A200, A300]
Remarks |