- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< It failed in transported to wrapper (518)

Error content | Failed to connect to the wrapping unit.
Detail | After the product was fed from the PS-AI to the wrapping unit, no wrapping demand occurred after the specified time had elapsed (unstable weighing).
Release method | Open the cover, remove the product, and press the [RETURN] button.
User’s action | Open the cover, remove the product, and press the [RETURN] button.
Service action |
Relevant locations | P-1105[A600]
Remarks |