- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Preparing film set (593－0001)

Error content | Preparing film set.
Detail | Message indicates that the insert plate is moving towards the film set position.
Solution | Clears automatically when the insert plate reached the film set position.
Action by user |
Action by service representative |
Related part |
Remarks | Sub-error 0001 is displayed when lower film is set.