< There is problem on wrapping controller (471)

Error content | Wrapper control board is abnormal.
Detail | An error occurred in the wrapper control board. Sub-error meanings are as follows: 0003: E2ROM writing error. 0088: IC for general-purpose communication error. 0999: High speed, external CPU reset interrupt.
Solution |
Action by user |
Action by service representative |
Related part | P-1105 [A100, A200, A300]
Remarks |