- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Battery is faulty (0106)

Error content | Battery is faulty.
Detail | Battery in the board is exhausted.
Solution | [OK] button
Action by user |
Action by service representative | Check the battery of the main board. Check the battery switch of the main board.
Related part | Main board
Remarks | Turn off the machine and replace the battery in the board. Confirm the battery switch.