- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< It cannot differentiate tray (0328)

Error content | Tray detection error.
Detail | Right and left sides of the tray are protruding. Lower side of the tray is protruding. Sub-error 0001 data abnormally
Solution | Fix tray placement, [OK] button
Action by user | Place the tray in the center again.
Action by service representative | Place the tray in the center again. Confirm the camera detection.
Related part | Main board, detection board
Remarks |